ph Treatment Tank Replacement

Description

In June 2026, in the process of troubleshooting the well pump, the pH Treatment Tank imploded.

It was discovered when this tank was bypassed flow increased from 5gpm to >15gpm.